{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["NI-2 эт"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"NI-2 эт","index":0,"n_rows":65,"n_cols":8,"rows_kept":65,"cut":false,"hidden":false,"merged":[[59,0,59,5],[40,0,40,5],[44,0,44,5],[1,0,1,5],[10,0,10,5],[24,0,24,5],[52,0,52,5]]}
["№","Наименование",null,"Количество","Состояние","Дополнительное описание"]
["PXI"]
[2,null,"Шасси PXI-1036",1,"новый"]
[3,"191332A-03","PXI-6221",1,"Б/У"]
[4,"191855C-02","PXI-6122",1,"Б/У"]
[5,null,"PXI Slot Blocker",4,"новое"]
[6,"188133J-01","PXI -7831R",1,"Б/У"]
[7,"188535D-01","PXI 8331",1,"Б/У"]
[8,null,"PXI MI06040E",1,"Б/У"]
[9,"193266A-01","PXI -8310 Stav Fabric + всякое",1,"после ремонта"]
["cRIO/sbRIO + модули"]
[10,null,"NI 9233",1,"Б/У","4-Channel, 14 S/s Aggregate, ±80 mV C Series Temperature Input Module",null,"958 евро"]
[11,null,"NI 9505",3,"Б/У","DC Brushed Servo Drive",null,"303 евро"]
[24,"166912D-01, 166912C-01, 166912C-01","NI 9233",3,"Б/У"]
[25,"198862A-01L","NI 9225",1,"Б/У","с разъёмом"]
[26,"198864B-01L, ---","NI-9211",2,"Б/У"]
[27,"198860A-01L","NI 9215",1,"Б/У","с разъёмом"]
[28,"189197F-01L","NI 9421",1,"Б/У"]
[29,"191316E-01L, 152182A-01L","NI-9401 ",3,"Б/У"]
[30,null," NI 9505",1,"Б/У"]
[31,"153371A-01L","NI 9694 + всякое",1,"б/у"]
[32,"141611A-01L","NI 9935 15pin",1,"Б/У"]
[33,null," 9237-prototip",2,"б/у "]
[34,"151628A-01L","Разъём 9924",1,"Б/У"]
["Кабели"]
[35,"190912-04","DB9M/DB15M/DB215M",1,"Б/У"]
[36,"184749С-01","1M",3,"Б/У"]
[37,"189041C-02","2M",2,"Б/У"]
[38,"189041-02","2М",1,"новый"]
[39,"187804B-01","1M",1,"Б/У"]
[40,"182873A",null,2,"Б/У"]
[41,"182869A",null,1,"Б/У"]
[42,182323,"1M",1,"Б/У"]
[43,"185095C-02","2M",1,"Б/У"]
[44,"1835698-01",null,1,"Б/У"]
[45,"192061B-01","кабель 1М",null,"Б/У"]
[46,"187678A-02","каб бел -2м",1,"Б/У"]
[47,195950,"RJ-50",7,"Б/У"]
[48,"192256A-01","кабель USB A/B 2.0",1,"Б/У"]
[49,null,"F-GEVP-5,0-P",1,"Б/У"]
["SCXI"]
[50,"185161A01","SCXI-1300",1,"Б/У"]
[51,"187009A-01","SCXI-1313",1,"Б/У"]
[52,"182360-01","SCXI-1121",1,"Б/У"]
["PCI"]
[53,"183480B-01","PCI-DIO-32HS",1,"Б/У"]
[54,"192463B-01","PCI-781XR",1,"Б/У"]
[55,"183800J-01","PCI-IMAQ-1408",1,"Б/У"]
[56,"191649C-04L","PCI 6518",2," Б/У СНЯТ С ПРО-ВА"]
[57,"192823B-01L","Фреймграббер PCIe-1427",1,"Б/У"]
[58,null,"PCI-8331",1,"Б/У"]
[59,"188513E-01L","PCI-GPIB с кабелем",1,"почти новый"]
["cFP"]
[60,"188539H-01","NI cFP-2000",1,"б/у","RT-контроллер линейки оборудования NI FieldPoint"]
[61,"188546B-01","NI cFP-BP-4",1,"б/у","4-слотовое шасси линейки оборудования NI FieldPoint с креплениями на стену"]
[62,"185837B-02","NI cFP-AI-111",2,"б/у","16-ти канальный модуль аналогового ввода, токовый сигнал 0 .. 20 мА, 16 бит"]
[63,"184105C-02","NI cFP-AI-110",1,"б/у","8-ми канальный модуль аналогового ввода, ток 0 .. 20 мА, напряжение мВ (В), 16 бит"]
[64,1872.08,"NI cFP-RTD-124",1,"б/у","8-ми канальный модуль  аналогового ввода, сигнал с выхода термосопротивления"]
[65,"188989A-01\n188989A-01\n188989C-01","NI cFP-CB-1",3,"б/у","конненкторный блок для  модулей линейки оборудования NI FieldPoint "]
["Разное"]
[66,"779687-01 ?","SC-2075",1,"Б/У"]
[67,"184677D-01","RS-232 8 port + кабель",1,"б/у"]
[68,"190177E","DAQPAD-6016",1,"сильно б/у "]
[69,"194929E-04L","USB-6251",1,"Б/У"]
[70,"185257A-01","корпус CA-1000",1,"Б/У"]